|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S.No** | **Specification** | **QTY** | **Price** | **Total** |
| 1 | 2MP Lite IR Fixed-focal Bullet Network Camera  2MP 1/2.8" CMOS image sensor, low luminance, and high definition image.  Outputs max. 2MP (1920 × 1080) @25/30 fps.  H.265 codec, high compression rate, ultra-low bit rate.Built-in IR LED, and the max. illumination distance is 30 m.ROI, SMART H.264+/H.265+, flexible coding, applicable to various bandwidth and storage environments.Rotation mode, WDR, 3D NR, HLC, BLC, digital watermarking, applicable to various monitoring scenes.Intelligent monitoring: Intrusion, tripwire. Abnormality detection: Motion detection, privacy masking, no SD card, SD card full, SD card error, network disconnection, IP conflict, illegal access, and voltage detection.Max. 256 G micro SD card.12V DC/PoE power supply.IP67 protection. | 42 indoor |  |  |
| 2 | Network Video Recorder (NVR) with 01 Tb HDD 16 channel IP Video Access SmartH.265+/H.265/SmartH.264+/H.264/MJPEG Max 320Mbps Incoming Bandwidth ·Up to 12MP Resolution for Preview and Playback HDMI/VGA simultaneous video output 3D intelligent positioning with Dahua PTZ camera | 03 |  |  |
|  | Network Video Recorder (NVR) with 01 Tb HDD 32 channel IP Video Access • Dual NIC Supports Multi-Address, Fault Tolerance, and Load Balance  • Smart H.265+ and Smart H.264+ Video Compression  • Maximum 320 Mbps Incoming Bandwidth  • Up to 12 MP Resolution for Preview and Playback  • Two (2) Gigabit Ethernet Connections  • Support for IPC and UPnP Protocols  • Customized Live View Layout with Support for Panoramic Displays  • Intelligent Video System with Business Analytics  • Compatible with Dahua Smart Motion Detection Cameras | 01 |  |  |
| 3 | 32 inch LED | 04 |  |  |
| 4 | PoE Switch 8 port | 07 |  |  |
| 5 | 2U Rack | 03 |  |  |
|  | Cat 6 cable 23- Gage | 03 |  |  |
| 6 | Chanal patti | APA |  |  |
|  | Power cable+light plugs+ adopters |  |  |  |
| 7 | Installation | 42Nos |  |  |
|  | **Total** |  |  |  |

***TENDER DOCUMENTS FOR CCTV CAMERAS***